EX. 5

16 BIT ADDITION

LHLD 2500

XCHG

LHLD 2502

MOV A,E

ADD L

MOV L,A

MOV A,D

ADC H

MOV H,A

SHLD 2504

HLT